Schedule of Requirements
STATEMENT OF NEED: 

Technical Specifications for Goods:

	Item No
	Minimum Technical Requirements
	Unit
	Quantity

	1
	4 MP Fixed Network Camera	Each
	17

	2
	8 MP IR Fixed Dome Network Camera	Each
	16

	3
	4 MP IR Fixed Bullet Network Camera	Each
	3

	4
	NVR 32-ch	Each
	2

	5
	[bookmark: _Hlk86748682]U/UTP Cat6 PVC 23 AWG Cable
	Each
	6

	6
	8 TB Purple Surveillance Hard Drive
	Each
	8

	7
	Installation, configuration, testing, training and documentation
	Each
	1



Item No (1): 4 MP Fixed Network Camera
	Camera

	Image Sensor
	1/2.8" Progressive Scan CMOS

	Min. Illumination
	Color: 0.001 Lux @ (F1.0, AGC ON)

	Shutter Speed
	1/3 s to 1/100,000 s

	Angle Adjustment
	Pan: 0° to 360°, tilt: 0° to 75°, rotate: 0° to 360°

	Slow Shutter
	Yes

	P/N
	P/N

	Wide Dynamic Range
	Digital WDR

	Lens

	Lens Type & FOV
	2.8 mm, horizontal FOV 107°, vertical FOV 56°, diagonal FOV 127°
4 mm, horizontal FOV 84°, vertical FOV 45°, diagonal FOV 99°

	Aperture
	F1.0

	Lens Mount
	M12

	Aperture Type
	Fixed

	Depth of Focus
	2.8 mm: 1.7 m to ∞
4 mm: 2.1 m to ∞

	Illuminator

	Smart Supplement Light
	Yes

	Supplement Light
	White

	White Light Range
	Up to 30 m

	Video

	Main Stream
	50Hz: 25fps (1920 × 1080, 1280 × 960, 1280 × 720)
60Hz: 30fps (1920 × 1080, 1280 × 960, 1280 × 720)

	Sub Stream
	50Hz: 25fps (640 × 480, 640 × 360, 320 × 240)
60Hz: 30fps (640 × 480, 640 × 360, 320 × 240)

	Video Compression
	Main stream: H.265+/H.265/H.264+/H.264
Sub-stream: H.265/H.264/MJPEG

	Video Bit Rate
	32 Kbps to 8 Mbps

	H.264 Type
	BaseLine Profile/Main Profile/High Profile

	H.265 Type
	Main Profile

	Region of Interest (ROI)
	1 fixed region for main stream

	Network

	Simultaneous Live View
	Up to 6 channels

	API
	ONVIF (PROFILE S, PROFILE G), ISAPI, SDK

	Protocols
	TCP/IP, ICMP, HTTP, FTP, DHCP, DNS, DDNS, RTP, RTSP, RTCP, NTP, UPnP, SMTP, IGMP,
QoS, IPv6, UDP, Bonjour, SSL/TLS

	User/Host
	Up to 32 users. 3 user levels: administrator, operator and user

	Security
	Password protection, complicated password, HTTPS encryption, IP address filter, security audit log, basic and digest authentication for HTTP/HTTPS, TLS 1.2, WSSE and digest authentication for ONVIF

	Client
	iVMS-4200, Hik-Connect, Hik-Central

	Web Browser
	Plug-in required live view: IE8, IE9, IE10, IE11
Local service: Chrome 57.0+, Firefox 52.0+

	Image

	Day/Night Switch
	Day, Night, Auto, Schedule

	Image Enhancement
	BLC, HLC, 3D DNR

	Image Settings
	Rotate mode, saturation, brightness, contrast, sharpness, gain, white balance
adjustable by client software or web browser

	Interface

	Communication Interface
	1 RJ45 10M/100M self-adaptive Ethernet port

	Intelligent (Traditional Algorithm)

	Basic Event
	Motion detection, exception (illegal login)

	General

	Linkage Method
	Upload to FTP/NAS, notify surveillance center, send email, trigger recording, trigger capture
*Note: External device is required.

	Web Client Language
	English

	General Function
	Anti- flicker, heartbeat, mirror, privacy masks, flash log, password reset via e-mail,
pixel counter

	Software Reset
	Reset via web browser and client software

	Power Supply
	12 VDC ± 25%, PoE: 802.3af, Type 1 Class 3, reverse polarity protection

	Power Consumption and
Current
	12 VDC, 0.30 A, max. 3.6 W
PoE (802.3af, 36 V to 57 V), 0.20 A to 0.10 A, max. 4.5W

	Power Interface
	Ø5.5 mm coaxial power plug

	Material
	Main body: metal; enclosure and base: plastic

	Camera Dimension
	Ø110 × 100.8 mm (4.3" × 4.0")

	Package Dimension
	150 × 150 × 141 mm (5.9" × 5.9" × 5.6")

	Camera Weight
	Approx. 350 g (0.7 lb.)

	With Package Weight
	Approx. 500 g (1.1 lb.)

	Approval

	EMC
	FCC (47 CFR Part 15, Subpart B); CE-EMC (EN 55032: 2015, EN 61000-3-2: 2014, EN
61000-3-3: 2013, EN 50130-4: 2011 +A1: 2014); RCM (AS/NZS CISPR 32: 2015); IC
(ICES-003: Issue 6, 2016); KC (KN 32: 2015, KN 35: 2015)

	Safety
	UL (UL 60950-1); CB (IEC 60950-1:2005 + Am 1:2009 + Am 2:2013); CE-LVD (EN 60950-1:2005 + Am 1:2009 + Am 2:2013); BIS (IS 13252(Part
1):2010+A1:2013+A2:2015)

	Environment
	CE-RoHS (2011/65/EU); WEEE (2012/19/EU); Reach (Regulation (EC) No 1907/2006)

	Protection
	Ingression protection: IP67 (IEC 60529-2013)



Item No (2): 8 MP IR Fixed Dome Network Camera 
	Camera

	Image Sensor
	1/2.5" Progressive Scan CMOS

	Min. Illumination
	Color: 0.01 lux @(F1.2, AGC ON), 0.028 lux @(F2.0, AGC ON), 0 lux with IR

	Shutter Speed
	1/3 s to 1/100,000 s

	Slow Shutter
	Yes

	Day & Night
	IR Cut Filter

	Digital Noise Reduction
	3D DNR

	WDR
	120dB

	3-Axis Adjustment
	Pan: 0° to 355°, tilt: 0° to 75°, rotate: 0° to 355°

	Lens

	Focal Length
	2.8/4/6/8 mm

	Aperture
	F2.0

	Focus
	Fixed

	FOV
	2.8 mm, horizontal FOV: 102°, vertical FOV: 53°, diagonal FOV: 124° 4 mm, horizontal FOV: 79°, vertical FOV: 42°, diagonal FOV: 95°
6 mm, horizontal FOV: 50°, vertical FOV: 28°, diagonal FOV: 59°
8 mm, horizontal FOV: 40°, vertical FOV: 25°, diagonal FOV: 53°

	Lens Mount
	M12

	IR
	

	IR Range
	Up to 30 m

	Wavelength
	850nm

	Compression: Standard

	Video Compression
	Main stream: H.265/H.264
Sub-stream: H.265/H.264/MJPEG
Third stream: H.265/H.264

	H.264 Type
	Main Profile/High Profile

	H.264+
	Main stream supports

	H.265 Type
	Main Profile

	H.265+
	Main stream supports

	Video Bit Rate
	32 Kbps to 16 Mbps

	Audio Compression (-S)
	G722.1/G.711/G726/MP2L2/PCM/MP3

	Audio Bit Rate (-S)
	64Kbps(G.711)/16Kbps(G.722.1)/16Kbps(G.726)/32-192Kbps(MP2L2)/8Kbps-320Kbps(MP3)

	Smart Feature-set

	Smart Event
	Line crossing detection, intrusion detection, face detection

	Basic Event
	Motion detection, video tampering alarm, exception (network disconnected, IP address  conflict, illegal login, HDD full, HDD error)

	Linkage Method
	Trigger recording: memory card, network storage, pre-record and post-record Trigger captured pictures uploading: FTP, HTTP, NAS, Email
Trigger notification: HTTP, ISAPI, alarm output (-S), Email

	Region of Interest
	Support 1 fixed region for main stream and sub-stream

	Image

	Max. Resolution
	3840 × 2160

	Main Stream
	50Hz: 12.5 fps (3840 × 2160), 20fps (3072 × 1728), 25 fps (2560 × 1440, 1920 × 1080, 1280 × 720)
60Hz: 15 fps (3840 × 2160), 20fps (3072 × 1728), 30 fps (2560 × 1440, 1920 × 1080, 1280 × 720)

	Sub-Stream
	50Hz: 25fps (640 × 480, 640 × 360, 320 × 240)
60Hz: 30fps (640 × 480, 640 × 360, 320 × 240)

	Third Stream
	50Hz: 25fps (1280 × 720, 640 × 360, 352 × 288)
60Hz: 30fps (1280 × 720, 640 × 360, 352 × 240)

	Image Enhancement
	BLC/3D DNR/HLC

	Image Setting
	Saturation, brightness, contrast, sharpness, AGC, and white balance adjustable by client software or web browser

	Target Cropping
	No

	Day/Night Switch
	Day/Night/Auto/Schedule/Triggered by Alarm In (-S)

	*Note: When the main stream resolution is 3840 × 2160, max frame rate is 12.5 fps (50Hz)/15 fps (60Hz) for all streams. When the main stream resolution is 3072 × 1728, max frame rate is 20 fps for all streams.

	Network

	Network Storage
	Support Micro SD/SDHC/SDXC card (128G), local storage and NAS (NFS,SMB/CIFS), ANR

	Protocols
	TCP/IP, UDP, ICMP, HTTP, HTTPS, FTP, DHCP, DNS, DDNS, RTP, RTSP, RTCP, PPPoE, NTP, UPnP, SMTP, SNMP, IGMP, 802.1X, QoS, IPv6, UDP, Bonjour, SSL/TLS

	General Function
	Anti-flicker, three streams, heartbeat, mirror, privacy masks, password reset via e-mail, pixel counter, HTTP listening

	API
	ONVIF (PROFILE S, PROFILE G, PROFILE T), ISAPI, SDK

	Security
	Password protection, complicated password, HTTPS encryption, 802.1X authentication (EAP-TLS 1.2,
EAP-LEAP, EAP-MD5), watermark, IP address filter, basic and digest authentication for HTTP/HTTPS, WSSE and digest authentication for ONVIF, TLS1.2

	Simultaneous Live View
	Up to 6 channels

	User/Host
	Up to 32 users
3 levels: Administrator, Operator and User

	Client
	iVMS-4200, Hik-Connect, Hik-Central

	Web Browser
	Plug-in required live view: IE8+
Plug-in free live view: Chrome 57.0+, Firefox 52.0+, Safari 11+ Local Service: Chrome 41.0+, Firefox 30.0+

	Interface
	 

	Audio (-S)
	1 input (line in/mic in), 1 output (line out), terminal block, mono sound

	Alarm (-S)
	1 input, 1 output (max. 12 VDC, 30 mA), terminal block

	Video Output
	No

	Communication Interface
	1 RJ45 10M/100M self-adaptive Ethernet port

	On-board Storage
	Built-in microSD/SDHC/SDXC slot, up to 128 GB

	SVC
	H.264 and H.265 encoding support

	Reset Button
	Yes

	Audio
	 

	Environment Noise Filtering
	Yes

	Audio Sampling Rate
	8 kHz/16 kHz/32 kHz/44.1 kHz/48 kHz

	General

	Operating Conditions
	-30 °C to +60 °C (-22 °F to +140 °F), humidity 95% or less (non-condensing)

	Web Client Language
	32 languages
English,  Russian,  Estonian,  Bulgarian,  Hungarian,  Greek,  German,  Italian,  Czech,  Slovak,  French,  Polish, Dutch, Portuguese, Spanish, Romanian, Danish, Swedish, Norwegian, Finnish, Croatian, Slovenian, Serbian, Turkish, Korean, Traditional Chinese, Thai, Vietnamese, Japanese, Latvian, Lithuanian, Portuguese (Brazil)

	Power Supply
	12 VDC ± 25%, Φ 5.5 mm coaxial power plug PoE(802.3af, class 3)

	Power Consumption and
	DC: 12 V, 0.6 A, max. 7.5 W

	Current
	PoE: (802.3af, 36 V to 57 V), 0.3 A to 0.2 A, max. 9 W

	Protection Level
	IP67, IK10

	Material
	Camera body: metal, bubble: plastic

	Dimensions
	Camera: Φ 111 mm × 82.4 mm (Φ 4.4" × 3.2")
Package: 134 × 134 × 108 mm (5.3" × 5.3" × 4.3")

	
	



Item No (3): 4 MP IR Fixed Bullet Network Camera
	Camera

	Image Sensor
	1/3" Progressive Scan CMOS

	Min. Illumination
	Color: 0.01 Lux @ (F1.2, AGC ON), 0.018 Lux @ (F1.6, AGC ON), 0 Lux with IR

	Shutter Speed
	1/3 s to 1/100,000 s

	Slow Shutter
	Yes

	Day & Night
	IR Cut Filter

	Digital Noise Reduction
	3D DNR

	WDR
	120dB

	3-Axis Adjustment
	Pan: 0° to 360°, tilt: 0° to 100°, rotate: 0° to 360°

	Lens

	Focal length
	2.8/4/6/8 mm

	Aperture
	F1.6

	Focus
	Fixed

	FOV
	2.8 mm, horizontal FOV: 103°, vertical FOV: 58°, diagonal FOV: 123° 4 mm, horizontal FOV: 83°, vertical FOV: 45°, diagonal FOV: 99°
6 mm, horizontal FOV: 51°, vertical FOV: 29°, diagonal FOV: 58°
8 mm, horizontal FOV: 39°, vertical FOV: 22°, diagonal FOV: 45°

	Lens Mount
	M12

	IR
	 

	IR Range
	-I5: Up to 50 m
-I8: Up to 80 m

	Wavelength
	850nm

	Compression Standard
	 

	Video Compression
	Main stream: H.265/H.264
Sub-stream: H.265/H.264/MJPEG
Third stream: H.265/H.264

	H.264 Type
	Main Profile/High Profile

	H.264+
	Main stream supports

	H.265 Type
	Main Profile

	H.265+
	Main stream supports

	Video Bit Rate
	32 Kbps to 16 Mbps

	Smart Feature-set
	 

	Smart Event
	Line crossing detection, intrusion detection, face detection

	Basic Event
	Motion detection, video tampering alarm, exception (network disconnected, IP address conflict, illegal login, HDD full, HDD error)

	Linkage Method
	Trigger recording: memory card, network storage, pre-record and post-record Trigger captured pictures uploading: FTP, HTTP, NAS, Email
Trigger notification: HTTP, ISAPI, Email

	Region of Interest
	1 fixed region for main stream and sub-stream

	Image

	Max. Resolution
	2688 × 1520

	Main Stream
	50Hz:25fps (2688 × 1520, 2560 × 1440, 2304 × 1296, 1920 × 1080, 1280 × 720)
60Hz: 30fps (2688 × 1520, 2560 × 1440, 2304 × 1296, 1920 × 1080, 1280 × 720)

	Sub-Stream
	50Hz: 25fps (640 × 480, 640 × 360, 320 × 240)
60Hz: 30fps (640 × 480, 640 × 360, 320 × 240)

	Third Stream
	50Hz: 25fps (1280 × 720, 640 × 360, 352 × 288)
60Hz: 30fps (1280 × 720, 640 × 360, 352 × 240)

	Image Enhancement
	BLC/3D DNR/HLC

	Image Setting
	Rotate mode, saturation, brightness, contrast, sharpness, AGC, and white balance are adjustable by client software or web browser

	Target Cropping
	No

	Day/Night Switch
	Day/Night/Auto/Schedule

	Network

	Network Storage
	Support Micro SD/SDHC/SDXC card (128G), local storage and NAS (NFS,SMB/CIFS), ANR

	Protocols
	TCP/IP, UDP, ICMP, HTTP, HTTPS, FTP, DHCP, DNS, DDNS, RTP, RTSP, RTCP, PPPoE, NTP, UPnP, SMTP, SNMP, IGMP, 802.1X, QoS, IPv6, UDP, Bonjour, SSL/TLS

	General Function
	Anti-flicker,  three  streams,  heartbeat,  mirror,  privacy  masks,  password  reset  via  e-mail,  pixel counter, HTTP listening

	Security
	Password protection, complicated password, HTTPS encryption, 802.1X authentication (EAP-TLS 1.2, EAP-LEAP, EAP-MD5), watermark, IP address filter, basic and digest authentication for HTTP/HTTPS, WSSE and digest authentication for ONVIF, TLS1.2

	API
	ONVIF (PROFILE S, PROFILE G, PROFILE T), ISAPI, SDK

	Simultaneous Live View
	Up to 6 channels

	User/Host
	Up to 32 users
3 levels: Administrator, Operator and User

	Client
	iVMS-4200, Hik-Connect, Hik-Central

	Web Browser
	Plug-in required live view: IE8+
Plug-in free live view: Chrome 57.0+, Firefox 52.0+, Safari 11+ Local Service: Chrome 41.0+, Firefox 30.0+

	Interface
	 

	Communication Interface
	1 RJ45 10M/100M self-adaptive Ethernet port

	Video Output
	No

	On-board storage
	Built-in Micro SD/SDHC/SDXC slot, up to 128 GB

	SVC
	H.264 and H.265 encoding

	Reset Button
	Yes

	General

	Operating Conditions
	-30 °C to +60 °C (-22 °F to +140 °F), Humidity 95% or less (non-condensing)

	Web Client Language
	32 languages
English,  Russian,  Estonian,  Bulgarian,  Hungarian,  Greek,  German,  Italian,  Czech,  Slovak,  French, Polish,  Dutch,  Portuguese,  Spanish,  Romanian,  Danish,  Swedish,  Norwegian,  Finnish,  Croatian, Slovenian,  Serbian,  Turkish,  Korean,  Traditional  Chinese,  Thai,  Vietnamese,  Japanese,  Latvian, Lithuanian, Portuguese (Brazil)

	Power Supply
	12 VDC ± 25%, Φ 5.5 mm coaxial power plug PoE (802.3af, class 3)

	Power Consumption and Current
	-I5:
12 VDC, 0.6 A, max. 7.5 W
PoE (802.3af, 36 V to 57 V), 0.2 A to 0.1 A, max. 9.5 W
-I8:
12 VDC, 0.95 A, max. 11.5 W
PoE (802.3af, 36 V to 57 V), 0.35 A to 0.1 A, max. 12.5 W

	Protection Level
	IP67

	Material
	Metal

	Dimensions
	Camera: Φ 105 × 299.7 mm (Φ 4.1" × 11.8")
Package: 386 × 156 × 155 mm (15.2" × 6.1" × 6.1")

	Weight
	Camera: Approx. 1180 g (2.6 lb.)
With Package: Approx. 1700 g (3.7 lb.)



Item No (4): NVR 32 channels
	Video/Audio input
	IP video input
	32-ch


	
	
	Up to 12 MP resolution

	
	Two-way audio
	1-ch, RCA (2.0 Vp-p, 1 k Ω)

	Network
	Incoming bandwidth
	320 Mbps

	
	
	or 200 Mbps (when RAID is enabled)

	
	Outgoing bandwidth
	256 Mbps, or 200 Mbps (when RAID is enabled)

	
	Remote connection
	128

	Video/Audio output
	Recording resolution
	12 MP/8 MP/6 MP/5 MP/4 MP/3 MP/1080p/UXGA/720p/VGA/4CIF/DCIF
/2CIF/CIF/QCIF

	
	CVBS output
(Optional)
	1-ch, BNC (1.0 Vp-p, 75 Ω), resolution: PAL: 704 × 576, NTSC: 704 × 480

	
	VGA1 /HDMI1 output resolution
	HDMI1:   4K   (3840   ×   2160)/60Hz,   4K   (3840   ×   2160)/30Hz,   2K   (2560   × 1440)/60Hz, 1920 × 1080p/60Hz, 1600 × 1200/60Hz, 1280 × 1024/60Hz, 1280
× 720/60Hz, 1024 × 768/60Hz

	
	
	VGA1: 2K (2560 × 1440)/60Hz, 1920 × 1080p/60Hz, 1600 × 1200/60Hz, 1280
× 1024/60Hz, 1280 × 720/60Hz, 1024 × 768/60Hz

	
	VGA2 /HDMI2 output resolution
	1920 × 1080p/60Hz, 1280 × 1024/60Hz, 1280 × 720/60Hz, 1024 × 768/60Hz

	
	Audio output
	2-ch, RCA (2.0Vp-p, 1 KΩ)

	Decoding
	Decoding format
	H.265/H.265+/H.264/H.264+/MPEG4

	
	Live        view/Playback resolution
	12 MP/8 MP/6 MP/5 MP/4 MP/3 MP/1080p/UXGA/720p/VGA/4CIF/DCIF
/2CIF/CIF/QCIF

	
	Synchronous playback
	16-ch

	
	Capability
	2-ch @ 12 MP (20fps) / 4-ch @ 8 MP (25fps) / 8-ch @ 4MP (30fps) / 16-ch @ 1080p (30fps)

	Network management
	Network protocols
	TCP/IP, DHCP, Hik-Connect, DNS, DDNS, NTP, SADP, SMTP, NFS, iSCSI, UPnP™, HTTPS

	Hard disk
	SATA
	8 SATA interfaces

	
	eSATA
	1 eSATA interface

	
	Capacity
	Up to 10TB capacity for each HDD

	Disk array
	Array type
	RAID0, RAID1, RAID5, RAID6, RAID10

	
	Number of arrays
	4

	External interface
	Network interface
	2, RJ-45 10/100/1000 Mbps self-adaptive Ethernet interface

	
	Serial interface
	RS-232; RS-485; Keyboard

	
	USB interface
	Front panel: 2 × USB 2.0; Rear panel: 1 × USB 3.0

	
	Alarm in/out
	16/4

	General
	Power supply
	100 to 240 VAC, 50 to 60 Hz

	
	Max. Power
	200 W

	
	Consumption (without hard disk)
	≤ 30 W

	
	Working temperature
	-10 °C to 55 °C (14 °F to 131 °F)

	
	Working humidity
	10 to 90 %

	
	Dimensions(W × D × H)
	445 × 470 ×90 mm (17.5"× 18.5" × 3.5")

	
	Weight
(without hard disk)
	≤ 10 kg (22 lb)




Item (5): U/UTP Cat6 PVC 23 AWG Cable
	Category
	Cat.6

	Sheath printing
	HIKVISION 4PR 23AWG 75°C U/UTP CAT6 VERIFIED TO ANSI/TIA-568-C.2 PVC ****m mm/dd/yyyy
Tracing Code-HS

	Reference standard
	ISO/IEC11801, ANSI/TIA-568-C.2, RoHS 2.0

	Fire resistance
	No

	Conductor
	Material
	Solid-Bare Copper (99.95%)

	
	Diameter
	0.55 ± 0.005 mm, 23 AWG

	Insulation
	Material
	HDPE

	
	Diameter
	0.98 ± 0.05 mm

	

Sheath
	Thickness
	0.50 ± 0.10 mm

	
	Diameter
	6.00 ± 0.30 mm

	
	Material
	PVC

	
	Color
	Orange

	Rip-cord
	Yes

	Separator
	Yes

	


Sheath physical properties
	
Before aging
	Tensile strength ≥ 13.5 Mpa
Elongation ≥ 150%

	
	Aging period
	100°C × 24h × 10d

	
	
After aging
	Tensile strength ≥ 12.5 Mpa

Elongation ≥ 125%

	
	Cold bend
	-20 ± 2°C × 4h, 8 × cable O.D, no visible cracks

	




Electrical

Characteristics (20°C)
	
1.0-250.0 MHz impedance
	100 ± 15 Ω @ ≤ 100 MHz

100 ± 25 Ω @100-250 MHz

	
	1.0-250.0 MHz delay skew
	≤ 45 ns/100 m

	
	DC resistance
	≤ 9.38 Ω/100 m

	
	DC conductor resistance unbalance
	≤ 5.0%

	
	Package dimension
	400 mm (W) × 400 mm (H) × 240 mm (D) (15.75" × 15.75" × 9.45")

	
	Weight
	12.3 ± 0.5kg

	
	Cable length
	(305 ± 1.5) m

	
	Ambient temperature
	-20°C to 75°C (-4°F to 167°F)

	
	Operating voltage
	60 V





Item (6): 8 TB Purple Surveillance Hard Drive 
	Capacity: 8 TB

	Interface: SATA

	Form Factor: 3.5 Inch

	Disk Speed (RPM): 7200rpm

	Compatibility: WD Purple™ surveillance storage is built to handle up to 64 cameras per drive and is designed for 24/7, always on, high-definition surveillance security systems with more than eight bays2.

	Dimensions (L x W x H): 5.79" x 4" x 1.03"




Item (7): Installation, configuration, testing, training and documentation
DELIVERY REQUIREMENTS: 

	Delivery Requirements

	Delivery date and time
	Vendor shall deliver the goods and install all required equipment within maximum of 15 days after PO issuance.

	Delivery Terms (INCOTERMS 2020)
	N/A

	Customs clearance
(Must be linked to INCOTERM)
	☒ Not applicable
Shall be done by:
☐ Name of organization
☐ Vendor/bidder
☐ Freight Forwarder

	Exact Address(es) of Delivery Location(s)
	Villa number 37, Street number 85, Maadi, Cairo, Egypt

	Distribution of shipping documents (if using freight forwarder)
	N/A

	Special Packing Requirements
	N/A


	Training on Operations and Maintenance
	Required

	Warranty Period
	1 Year

	After-sales service and local service support requirements
	Not Required

	Preferred Mode of Transport
	Land


	Subcontracting
	The vendor is strongly encouraged not to sub-contract > 50% of the total work. If a vendor/s intend to do so, they must state the actual percentage (that will be outsourced) in their offer/quotation.



INSPECTIONS AND TESTS:
The following inspections and tests shall be performed:
· Test the items and ensure that all system and its items are properly installed and configured, orientation and written documentation with drawings is needed.
· If the goods fail to meet the laid down specifications, the vendor shall take immediate steps to remedy the deficiency or replace the defective goods to the satisfaction of UN Women.



